#
OIL COOLER REMOVAL/INSTALLATION [L3]

BME011114700201

1. Disconnect the negative battery cable.

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS.)(See ENGINE COOLANT REPLACEMENT [L3].)

3. Remove in the order indicated in the table.

4. Install in the reverse order of the removal.

1 | Water hose
2 | Oil cooler

5. Refill the engine coolant. (See ENGINE COOLANT REPLACEMENT [L3].)

6. Inspect the oil level.

  • If necessary, add oil. (See ENGINE OIL LEVEL INSPECTION.)

7. Start the engine and inspect for oil leakage.

  • If the oil leaks, specify the faulty part and repair or replace it.