#
INTAKE MANIFOLD COMMUNICATION CONTROL (IMCC) SYSTEM OUTLINE [AJ]

BME011300045T01
• Due to the adoption of an IMCC system, higher engine torque has been obtained at all engine speeds.
• The IMCC system concept is the same as the variable resonance induction system (VRIS).

1 | IMCC open
2 | IMCC close
3 | IMCC valve close
4 | IMCC valve open
5 | Approx 3,750 rpm
6 | Approx 5,560 rpm
7 | Engine torque
8 | Engine speed
9 | High
10 | Low