#
POWER WINDOW MOTOR INSPECTION

BME091259560201

## Driver's Side

1. Remove the power window motor. (See FRONT POWER WINDOW REGULATOR DISASSEMBLY/ASSEMBLY.)

2. Apply battery positive voltage to the power window motor terminals A and G and inspect the operation of the power window motor.

  • If not as specified, replace the power window motor.

Terminal | Motor operation
--- | ---
A | G
GND | B+ | UP
B+ | GND | DOWN

3. Apply 5 V to the power window motor terminal B and connect terminal F to ground.

4. Measure the voltage at terminal D while operating the power window motor.

  • If not as specified, replace the power window motor.

Voltage

  Pulse wave: MAX. 5 V, MIN. 0 V

## Except Driver's Side

1. Remove the power window motor.

2. Apply battery positive voltage to the power window motor terminals and inspect the operation of the power window motor.

  • If not as specified, replace the power window motor.

Terminal | Motor operation
--- | ---
A | B
GND | B+ | UP
B+ | GND | DOWN