#
FOREWORD [AJ]

BME010300103202
• When the customer reports a vehicle malfunction, inspect the malfunction indicator lamp (MIL) indication and diagnostic trouble code (DTC), then diagnose the malfunction according to the following flowchart.

  - If a DTC exists, diagnose the applicable DTC inspection. (See DTC TABLE [AJ] (VIN: JMZ LW19J7*# 300001-, JM0 LW10J300 300001-301405, JM6 LW10J300 300001-, JM8 LW28J**# 300001-301513).)(See DTC TABLE [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
  - If no DTC exists and the MIL does not illuminate or flash, diagnose the applicable symptom troubleshooting. (See SYMPTOM DIAGNOSTIC INDEX [AJ].)

*: Malfunction Indicator Lamp (MIL), Generator Warning Light, Security Light