#
BASIC SYSTEM FLOW DIAGRAM

BME071100000T02

## Front

• When the A/C is turned on, the air that passes through the air filter and front blower motor is cooled, dehumidified, and filtered by the front evaporator, then heated by the front heater core.
• The ventilation of the second-row seat is improved using rear heat duct.
• The side windows are defrosted by ventilation from the side demister.

.

1 | Center vent
2 | Side vent
3 | Front heat
4 | Rear heat
5 | Defroster and side demister
6 | Blower unit
7 | Front A/C unit
8 | Rear heat duct component (for second-row seat)

## Rear

• When the A/C is turned on, the air that passes through the rear blower motor is cooled, dehumidified, and filtered by the rear evaporator, then heated by the rear heater core.

.

1 | Roof vent
2 | Rear heat
3 | Rear A/C unit
4 | Rear cooler duct
5 | Rear heat duct component (for third-row seat)