#
SOLENOID VALVE REMOVAL/INSTALLATION [JA5A-EL]

BME051721280204

1. Remove the control valve body. (See CONTROL VALVE BODY REMOVAL/INSTALLATION [JA5A-EL].)

2. Remove the solenoid valves and manual valve.

1 | Manual valve
2 | 2-4 brake solenoid valve
3 | Neutral shift solenoid valve
4 | TCC solenoid valve
5 | Shift solenoid C
6 | Shift solenoid B
7 | Reduction timing solenoid valve
8 | Shift solenoid A
9 | Pressure control solenoid
10 | High clutch solenoid valve

3. Apply ATF to a new O-ring and install it on the solenoid valve.

4. Install the solenoid valve and manual valve in the control valve body.

Tightening torque

  8.34-10.30 N·m {85-105 kgf·cm, 74-91 in·lbf}

5. Install the control valve body. (See CONTROL VALVE BODY REMOVAL/INSTALLATION [JA5A-EL].)

6. Add the ATF while the engine is idling, and inspect the ATF level and leakage. (See AUTOMATIC TRANSAXLE FLUID (ATF) REPLACEMENT [JA5A-EL].) (See Automatic Transaxle Fluid (ATF) Level Inspection.)

7. Perform the time lag test and line pressure test. (See MECHANICAL SYSTEM TEST [JA5A-EL].)