#
COIL REMOVAL/INSTALLATION

BME091467004201

  Note

  • Do not remove the coil unless you are replacing it.
  • When only the coil is replaced, the immobilizer system reprogram procedure is not necessary.

1. Disconnect the negative battery cable.

2. Remove the column cover.

3. Remove in the order indicated in the table.

4. Install in the reverse order of removal.

1 | Connector
2 | Coil (See Coil Installation Note.)

## Coil Installation Note

1. Install the hook 1 to the steering lock.

2. Install the hook 2 to the steering lock.