#
BRAKES TECHNICAL DATA

BME045001020201

Item | Specification
--- | ---
CONVENTIONAL BRAKE SYSTEM
Brake pedal | Brake pedal height | (mm {in}) | 210 {8.27} (reference value)
Brake pedal play | (mm {in}) | 7.8-12.0 {0.31-0.47}
Pedal-to-floor clearance | (mm {in}) | 113 {4.45} min.
Power brake unit | Fluid pressure | At 0 kPa {0 mmHg, 0 inHg} | 680 {6.93, 98.6} min.
(kPa {kgf/cm2, psi}) | At 66.7 kPa {500 mmHg, 19.7 inHg} | 8,900 {90.75, 1,291} min.
Front disc brake | Minimum disc pad thickness | (mm {in}) | 2.0 {0.08}
Minimum disc plate thickness | (mm {in}) | 26 {1.03}
Disc plate runout limit | (mm {in}) | 0.05 {0.002}
Rear disc brake | Minimum disc pad thickness | (mm {in}) | 2.0 {0.08}
Minimum disc plate thickness | (mm {in}) | 16 {0.63}
Disc plate runout limit | (mm {in}) | 0.05 {0.002}
Brake fluid | Type | European (L.H.D. U.K.) specs: SAE J1703, FMVSS116 DOT-3 OR DOT-4 Except European (L.H.D. U.K.) specs: SAE J1703, FMVSS116 DOT-3
PARKING BRAKE SYSTEM
Parking brake lever | Lever stroke when pulled at 98 N {10 kgf, 22 lbf} | (notches) | 5 max. (no drag)
Parking drum brake (Vehicles with rear disc brake) | Maximum brake drum diameter | (mm {in}) | 190.0 {7.48}
Minimum lining thickness | (mm {in}) | 1.0 {0.04}
Clearance between shoe and drum | Manual adjuster