#
THIRD-ROW SEAT INSTALLATION

BME09135730XW02

## TYPE A

1. Set the seat's strikers on the rear floor anchor loops.

2. Lower the seat forward to lock the front strikers.

3. Supporting the seat with your hands, slowly lower the seat back rearwards to lock it in place.

4. Raise the recliner lever and raise the seat back upright.

5. Inspect the seat to ensure it is firmly locked in place.

## TYPE B

### Seat

1. Install in the reverse order of removal.

### Hinge

1. Install in the reverse order of removal.

### Striker

1. Install in the reverse order of removal.