#
OIL COOLER REMOVAL/INSTALLATION [AJ]

BME011114700202

1. Disconnect the negative battery cable.

2. Drain the engine coolant. (See COOLING SYSTEM SERVICE WARNINGS.)(See ENGINE COOLANT REPLACEMENT [AJ].)

3. Remove the oil filter. (See OIL FILTER REPLACEMENT [AJ].)

4. Remove in the order indicated in the table.

5. Install in the reverse order of removal.

1 | Water hose
2 | Oil cooler (See Oil Cooler Installation Note.)

6. Refill the engine coolant. (See ENGINE COOLANT REPLACEMENT [AJ].)

7. Inspect the engine oil level.

  • If necessary, add oil. (See ENGINE OIL LEVEL INSPECTION.)

8. Start the engine and inspect for oil leakage.

  • If the oil leaks, specify the faulty part and repair or replace it.

## Oil Cooler Installation Note

1. Install the locating pin on the oil cooler into the cast slot in the cylinder block.

2. Rotate the oil cooler clockwise until the cooler stops.