#
PRIMARY SHAFT COMPONENTS PREINSPECTION

BME051517201M01

## 3rd Gear Thrust Clearance

1. Measure the clearance between the 3rd gear and 2nd gear.

  • If not within the specification, assemble the primary shaft component again.

Clearance

  0.18-0.31 mm {0.0071-0.0122 in}

## 5th Gear Thrust Clearance

1. Measure the clearance between 4th thrust washer and the 5th gear.

  • If not within the specification, assemble the primary shaft component again.

Clearance

  0.06-0.16 mm {0.0024-0.0063 in}

## 4th Gear End Play

1. Remove the primary shaft rear bearing.

2. Set up the primary shaft component, and fix it.

3. Slide the 4th gear up and down, and measure the length of the movement.

  • If not within the specification, assemble the primary shaft component again.

Length of the movement

  0.20-0.30 mm {0.0078-0.0118 in}