#
INTERMEDIATE SENSOR DESCRIPTION [JA5A-EL]

BME051719200T09

## Function

• A intermediate sensor is located in the transaxle case and detects the rotating speed of the output gear.

## Construction/Operation

• The magnetic pickup type of intermediate sensor is mounted in the transaxle case, next to the output gear. It generates a 54-pulse signal for each rotation of the output gear, and sends this signal to the TCM.