#
DTC P0661 [AJ]

BME010200600W03

DTC P0661 | Intake manifold communication control (IMCC) circuit low input
--- | ---
DETECTION CONDITION | • The PCM monitors the IMCC actuator control signal at PCM terminal 97. If the PCM turns IMCC actuator off but voltage at PCM terminal 97 still remains low, the PCM determines that IMCC actuator circuit has malfunction. Diagnostic support note
• This is a continuous monitor (Other).
• The MIL illuminates if the PCM detects the above malfunction condition in the first drive cycle.
• PENDING CODE is available if the PCM detects the above malfunction condition.
• The FREEZE FRAME DATA is not available.
• The DTC is stored in the PCM memory.
POSSIBLE CAUSE | • IMCC actuator malfunction • Open circuit in wiring harness between main relay and IMCC actuator terminal A • Open circuit in wiring harness between IMCC actuator terminal B and PCM terminal 97 • Short to ground in wiring harness between IMCC actuator terminal B and PCM terminal 97
• Connector or terminal malfunction
• PCM malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | VERIFY FREEZE FRAME DATA HAS BEEN RECORDED • Has FREEZE FRAME DATA been recorded? | Yes | Go to the next step.
No | Record the FREEZE FRAME DATA on the repair order, then go to the next step.
2 | VERIFY RELATED REPAIR INFORMATION AVAILABILITY • Verify related Service Information and/or on-line repair information availability. • Is any related repair information available? | Yes | Perform repair or diagnosis according to the available repair information. • If the vehicle is not repaired, go to the next step.
No | Go to the next step.
3 | INSPECT IMCC ACTUATOR CONNECTOR FOR POOR CONNECTION • Turn the ignition switch off. • Disconnect the IMCC actuator connector. • Inspect for poor connection (damaged/pulled-out pins, corrosion, etc.). • Is there malfunction? | Yes | Repair or replace the terminal, then go to Step 9.
No | Go to the next step.
4 | INSPECT IMCC ACTUATOR MALFUNCTION • Inspect the IMCC actuator. (See INTAKE MANIFOLD COMMUNICATION CONTROL (IMCC) ACTUATOR INSPECTION [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).) • Is the IMCC actuator normal? | Yes | Go to the next step.
No | Replace the IMCC actuator, then go to step 9.
5 | INSPECT IMCC ACTUATOR POWER SUPPLY CIRCUIT FOR OPEN CIRCUIT • Turn the ignition switch to the ON position (Engine off). • Measure the voltage between IMCC actuator terminal A (wiring harness-side) and body ground. • Is the voltage B+? | Yes | Go to the next step.
No | Repair or replace the wiring harness for open, then go to Step 9.
6 | INSPECT IMCC ACTUATOR CONTROL CIRCUIT FOR SHORT TO GROUND • Inspect for continuity between IMCC actuator terminal B (wiring harness-side) and body ground. • Is there continuity? | Yes | Repair or replace the wiring harness for short to ground, then go to Step 9.
No | Go to the next step.
7 | INSPECT PCM CONNECTOR FOR POOR CONNECTION • Disconnect the PCM connector. • Inspect for poor connection at terminal 97. (damaged/pulled-out pins, corrosion, etc.). • Is there any malfunction? | Yes | Repair the terminal, then go to Step 9.
No | Go to the next step.
8 | INSPECT IMCC ACTUATOR CONTROL CIRCUIT FOR OPEN • Inspect for continuity between IMCC actuator terminal B (wiring harness-side) and PCM terminal 97 (wiring harness-side). • Is there continuity? | Yes | Go to the next step.
No | Repair or replace the wiring harness for open circuit, then go to the next step.
9 | VERIFY TROUBLESHOOTING OF DTC P0661 COMPLETED • Make sure to reconnect all disconnected connectors. • Turn the ignition switch to the ON position (Engine off). • Clear the DTC from the PCM memory using the WDS or equivalent. • Access RPM PID.
• Increase the engine speed 3,800 rpm or more for 10 times.
• Is the same DTC present?
Yes
Replace the PCM, then go to the next step.
(See PCM REMOVAL/INSTALLATION [AJ].)
No | Go to the next step.
10 | VERIFY AFTER REPAIR PROCEDURE • Perform the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [AJ].) • Is any DTC present? | Yes | Go to the applicable DTC troubleshooting. (See DTC TABLE [AJ] (VIN: JM0 LW10J300 301406-, JMZ LW69J7*# 307683-, JM8 LW28J**# 301514-, JM8 LW28A**# 301514- (Assumed)).)
No | Troubleshooting completed.