#
AIR FILTER INSPECTION

BME071161140W04

1. Remove the air filter.

2. Inspect for damage, excessive dirt, or foul smell.

  • If the air filter is damaged, excessively dirty, or foul smelling, replace it.

  Note

  • Replace the air filter once a year or at after every following mileage, depending on operating conditions.

  - Europe (L.H.D. U.K.): 15,000 km {9,000 miles}

  • The air filter cannot be reused by cleaning it with water or compressed air.