#
DTC TABLE [MZR-CD (RF Turbo)]

BME010200102235
×: Applicable -: Not applicable

DTC | Condition | MIL | DC | Memory function | Page
--- | --- | --- | --- | --- | ---
P0016 | Crankshaft position-camshaft position correlation malfunction | ON | 2 | × | (See DTC P0016 [MZR-CD (RF Turbo)])
P0045 | Variable boost control (VBC) solenoid valve control circuit low or high input | ON | 2 | × | (See DTC P0045 [MZR-CD (RF Turbo)])
P0088 | Fuel pressure system too high | - | - | × | (See DTC P0088 [MZR-CD (RF Turbo)])
P0093 | Fuel system leak detection | ON | 1 | × | (See DTC P0093 [MZR-CD (RF Turbo)])
P0096 | Intake air temperature (IAT) sensor No.2 range/performance problem | ON | 2 | × | (See DTC P0096 [MZR-CD (RF Turbo)])
P0097 | Intake air temperature (IAT) sensor No.2 circuit low input | ON | 1 | × | (See DTC P0097 [MZR-CD (RF Turbo)])
P0098 | Intake air temperature (IAT) sensor No.2 circuit high input | ON | 1 | × | (See DTC P0098 [MZR-CD (RF Turbo)])
P0101 | Mass air flow (MAF) sensor range/performance problem | ON | 2 | × | (See DTC P0101 [MZR-CD (RF Turbo)])
P0102 | Mass air flow (MAF) sensor circuit low input | ON | 1 | × | (See DTC P0102 [MZR-CD (RF Turbo)])
P0103 | Mass air flow (MAF) sensor circuit high input | ON | 1 | × | (See DTC P0103 [MZR-CD (RF Turbo)])
P0106 | Boost sensor range/performance problem | ON | 2 | × | (See DTC P0106 [MZR-CD (RF Turbo)])
P0107 | Boost sensor circuit low input | ON | 1 | × | (See DTC P0107 [MZR-CD (RF Turbo)])
P0108 | Boost sensor circuit high input | ON | 1 | × | (See DTC P0108 [MZR-CD (RF Turbo)])
P0111 | Intake air temperature (IAT) sensor No.1 range/performance problem | ON | 2 | × | (See DTC P0111 [MZR-CD (RF Turbo)])
P0112 | Intake air temperature (IAT) sensor No.1 circuit low input | ON | 1 | × | (See DTC P0112 [MZR-CD (RF Turbo)])
P0113 | Intake air temperature (IAT) sensor No.1 circuit high input | ON | 1 | × | (See DTC P0113 [MZR-CD (RF Turbo)])
P0116 | Engine coolant temperature (ECT) sensor range/performance problem | ON | 2 | × | (See DTC P0116 [MZR-CD (RF Turbo)])
P0117 | Engine coolant temperature (ECT) sensor circuit low input | ON | 1 | × | (See DTC P0117 [MZR-CD (RF Turbo)])
P0118 | Engine coolant temperature (ECT) sensor circuit high input | ON | 1 | × | (See DTC P0118 [MZR-CD (RF Turbo)])
P0122 | Accelerator pedal position (APP) sensor No.1 circuit low input | ON | 1 | × | (See DTC P0122 [MZR-CD (RF Turbo)])
P0123 | Accelerator pedal position (APP) sensor No.1 circuit high input | ON | 1 | × | (See DTC P0123 [MZR-CD (RF Turbo)])
P0182 | Fuel temperature sensor circuit low input | ON | 1 | × | (See DTC P0182 [MZR-CD (RF Turbo)])
P0183 | Fuel temperature sensor circuit high input | ON | 1 | × | (See DTC P0183 [MZR-CD (RF Turbo)])
P0191 | Fuel pressure sensor range/performance problem | ON | 2 | × | (See DTC P0191 [MZR-CD (RF Turbo)])
P0192 | Fuel pressure sensor circuit low input | ON | 1 | × | (See DTC P0192 [MZR-CD (RF Turbo)])
P0193 | Fuel pressure sensor circuit high input | ON | 1 | × | (See DTC P0193 [MZR-CD (RF Turbo)])
P0200 | Fuel injector operation identified | ON | 1 | × | (See DTC P0200 [MZR-CD (RF Turbo)])
P0201 | Fuel injector No.1 operation identified | ON | 1 | × | (See DTC P0201 [MZR-CD (RF Turbo)])
P0202 | Fuel injector No.2 operation identified | ON | 1 | × | (See DTC P0202 [MZR-CD (RF Turbo)])
P0203 | Fuel injector No.3 operation identified | ON | 1 | × | (See DTC P0203 [MZR-CD (RF Turbo)])
P0204 | Fuel injector No.4 operation identified | ON | 1 | × | (See DTC P0204 [MZR-CD (RF Turbo)])
P0222 | Accelerator pedal position (APP) sensor No.2 circuit low input | ON | 1 | × | (See DTC P0222 [MZR-CD (RF Turbo)])
P0223 | Accelerator pedal position (APP) sensor No.2 circuit high input | ON | 1 | × | (See DTC P0223 [MZR-CD (RF Turbo)])
P0225 | Idle switch circuit malfunction | ON | 2 | × | (See DTC P0225 [MZR-CD (RF Turbo)])
P0301 | Cylinder No.1 misfire detection | ON | 1 | × | (See DTC P0301, P0302, P0303, P0304 [MZR-CD (RF Turbo)])
P0302 | Cylinder No.2 misfire detection | ON | 1 | × | (See DTC P0301, P0302, P0303, P0304 [MZR-CD (RF Turbo)])
P0303 | Cylinder No.3 misfire detection | ON | 1 | × | (See DTC P0301, P0302, P0303, P0304 [MZR-CD (RF Turbo)])
P0304 | Cylinder No.4 misfire detection | ON | 1 | × | (See DTC P0301, P0302, P0303, P0304 [MZR-CD (RF Turbo)])
P0336 | CKP sensor range/performance problem | ON | 2 | × | (See DTC P0336 [MZR-CD (RF Turbo)])
P0337 | CKP sensor circuit low input | ON | 1 | × | (See DTC P0337 [MZR-CD (RF Turbo)])
P0341 | CMP sensor range/performance problem | ON | 2 | × | (See DTC P0341 [MZR-CD (RF Turbo)])
P0342 | CMP sensor circuit low input | ON | 1 | × | (See DTC P0342 [MZR-CD (RF Turbo)])
P0401 | EGR flow insufficient detected | ON | 2 | × | (See DTC P0401 [MZR-CD (RF Turbo)])
P0402 | EGR flow excessive detected | ON | 2 | × | (See DTC P0402 [MZR-CD (RF Turbo)])
P0404 | EGR valve stuck | ON | 2 | × | (See DTC P0404 [MZR-CD (RF Turbo)])
P0406 | EGR valve position sensor circuit high input | ON | 1 | × | (See DTC P0406 [MZR-CD (RF Turbo)])
P0489 | EGR solenoid valve (vacuum) control circuit low input | ON | 2 | × | (See DTC P0489 [MZR-CD (RF Turbo)])
P0490 | EGR solenoid valve (vacuum) control circuit high input | ON | 2 | × | (See DTC P0490 [MZR-CD (RF Turbo)])
P0500 | Vehicle speed signal (VSS) circuit malfunction | ON | 2 | × | (See DTC P0500 [MZR-CD (RF Turbo)])
P0512 | Engine switch circuit high input | ON | 1 | × | (See DTC P0512 [MZR-CD (RF Turbo)])
P0562 | Battery voltage low input | ON | 1 | × | (See DTC P0562 [MZR-CD (RF Turbo)])
P0563 | Battery voltage high input | ON | 1 | × | (See DTC P0563 [MZR-CD (RF Turbo)])
P0606 | PCM malfunction | ON | 1 | × | (See DTC P0606 [MZR-CD (RF Turbo)])
P0627 | Suction control valve circuit open | ON | 1 | × | (See DTC P0627 [MZR-CD (RF Turbo)])
P0628 | Suction control valve circuit low input | ON | 1 | × | (See DTC P0628 [MZR-CD (RF Turbo)])
P0629 | Suction control valve circuit high input | ON | 1 | × | (See DTC P0629 [MZR-CD (RF Turbo)])
P0661 | Intake shutter solenoid valve (half) circuit low input | ON | 2 | × | (See DTC P0661 [MZR-CD (RF Turbo)])
P0662 | Intake shutter solenoid valve (half) circuit high input | ON | 2 | × | (See DTC P0662 [MZR-CD (RF Turbo)])
P0664 | Intake shutter solenoid valve (full) circuit voltage low input | ON | 2 | × | (See DTC P0664 [MZR-CD (RF Turbo)])
P0665 | Intake shutter solenoid valve (full) circuit voltage high input | ON | 2 | × | (See DTC P0665 [MZR-CD (RF Turbo)])
P0704 | Clutch pedal position switch circuit malfunction | ON | 2 | × | (See DTC P0704 [MZR-CD (RF Turbo)])
P0850 | Neutral switch circuit malfunction | ON | 2 | × | (See DTC P0850 [MZR-CD (RF Turbo)])
P1190 | Calibration resistor circuit malfunction | ON | 2 | × | (See DTC P1190 [MZR-CD (RF Turbo)])
P1211 | Fuel pressure higher or lower than desired pressure | ON | 2 | × | (See DTC P1211 [MZR-CD (RF Turbo)])
P1391 | Glow plug circuit low input | - | - | × | (See DTC P1391 [MZR-CD (RF Turbo)])
P1392 | Glow plug circuit high input | - | - | × | (See DTC P1392 [MZR-CD (RF Turbo)])
P1602 | Immobilizer unit-PCM communication error | - | - | - | (See DTC P1602 [MZR-CD (RF Turbo)])
P1603 | Key ID number unregistered in PCM | - | - | - | (See DTC P1603 [MZR-CD (RF Turbo)])
P1604 | Code word unregistered in PCM | - | - | - | (See DTC P1604 [MZR-CD (RF Turbo)])
P1621 | Code words do not match after engine cranking | - | - | - | (See DTC P1621 [MZR-CD (RF Turbo)])
P1622 | Key ID number mismatch | - | - | - | (See DTC P1622 [MZR-CD (RF Turbo)])
P1623 | Cord word or key ID number read/write error in PCM | - | - | - | (See DTC P1623 [MZR-CD (RF Turbo)])
P1624 | Immobilizer system communication counter = 0 | - | - | - | (See DTC P1624 [MZR-CD (RF Turbo)])
P1675 | Fuel injector code unprogrammed | ON | 1 | × | (See DTC P1675 [MZR-CD (RF Turbo)])
P1676 | Fuel injector code incorrectly programmed | ON | 1 | × | (See DTC P1676 [MZR-CD (RF Turbo)])
P2009 | Variable swirl control (VSC) solenoid valve circuit high input | ON | 2 | × | (See DTC P2009 [MZR-CD (RF Turbo)])
P2010 | Variable swirl control (VSC) solenoid valve circuit low input | ON | 2 | × | (See DTC P2010 [MZR-CD (RF Turbo)])
P2135 | Accelerator pedal position (APP) sensor No.1/No.2 voltage correlation | ON | 1 | × | (See DTC P2135 [MZR-CD (RF Turbo)])
P2136 | Accelerator pedal position (APP) sensor No.1/idle switch correlation | ON | 1 | × | (See DTC P2136 [MZR-CD (RF Turbo)])
P2141 | EGR solenoid valve (vent) circuit low input | ON | 2 | × | (See DTC P2141 [MZR-CD (RF Turbo)])
P2142 | EGR solenoid valve (vent) circuit high input | ON | 2 | × | (See DTC P2142 [MZR-CD (RF Turbo)])
P2144 | EGR solenoid valve circuit low input | ON | 2 | × | (See DTC P2144 [MZR-CD (RF Turbo)])
P2145 | EGR solenoid valve circuit high input | ON | 2 | × | (See DTC P2145 [MZR-CD (RF Turbo)])
P2146 | Fuel injector No.1/No.4 circuit malfunction | ON | 1 | × | (See DTC P2146 [MZR-CD (RF Turbo)])
P2149 | Fuel injector No.2/No.3 circuit malfunction | ON | 1 | × | (See DTC P2149 [MZR-CD (RF Turbo)])
P2227 | BARO sensor range/performance problem | ON | 2 | × | (See DTC P2227 [MZR-CD (RF Turbo)])
P2228 | BARO sensor circuit low input | ON | 1 | × | (See DTC P2228 [MZR-CD (RF Turbo)])
P2229 | BARO sensor circuit high input | ON | 1 | × | (See DTC P2229 [MZR-CD (RF Turbo)])
U0073 | CAN BUS OFF | - | - | × | (See DTC U0073 [MZR-CD (RF Turbo)])
U0121 | Lost communication with ABS (ABS/TCS) HU/CM | - | - | × | (See DTC U0121 [MZR-CD (RF Turbo)])
U0166 | Lost communication with auxiliary heater control module | - | - | × | (See DTC U0166 [MZR-CD (RF Turbo)])