#
FRONT STABILIZER REMOVAL/INSTALLATION

BME021334100W01

1. Remove the crossmember. (See FRONT CROSSMEMBER REMOVAL/INSTALLATION.)

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

4. Inspect the front wheel alignment and adjust it as necessary. (See FRONT WHEEL ALIGNMENT.)

1 | Stabilizer control link
2 | Stabilizer bracket (See Stabilizer Bracket Installation Note.)
3 | Stabilizer bushing
4 | Front stabilizer

## Stabilizer Bracket Installation Note

1. Apply rubber grease to the inside surface of the stabilizer bushing.

2. Align the bushing with the inside of positioning plate on the stabilizer bar.

3. Install the stabilizer bracket.