#
INPUT/TURBINE SPEED SENSOR REMOVAL/INSTALLATION [JA5A-EL]

BME051721550202

1. Remove the automatic transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].)

2. Remove the input/turbine speed sensor. (See Automatic Transaxle Workshop Manual JA5A-EL.)

3. Install the input/turbine speed sensor. (See Automatic Transaxle Workshop Manual JA5A-EL.)

4. Install the automatic transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].)