#
REAR OIL SEAL REPLACEMENT [AJ]

BME011011399204

1. Remove the automatic transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].)

2. Remove the drive plate. (See DRIVE PLATE REMOVAL/INSTALLATION [JA5A-EL].)

3. Cut the oil seal lip using a razor knife.

4. Remove the rear oil seal using a screwdriver as shown.

5. Install the rear oil seal with part A of the SST [303-178 (49 UN01 070)] and the SST [303-384 (49 UN30 3384)].

6. Install the studs of the SST [303-384 (49 UN30 3384)] as indicated in the figure.

7. Apply clean engine oil to the oil seal.

8. Push the oil seal slightly in by hand.

9. Install part A of the SST [303-178 (49 UN01 070)] and compress the oil seal with the nuts of the SST [303-384 (49 UN30 3384)].

10. Install the drive plate. (See DRIVE PLATE REMOVAL/INSTALLATION [JA5A-EL].)

11. Install the automatic transaxle. (See AUTOMATIC TRANSAXLE REMOVAL/INSTALLATION [JA5A-EL].)