#
DTC 06 ERR10 OR 06:ER10

BME090266900W10

DTC 06 ERR10 or 06:Er10 | CD changer (upper module)-base unit communication line
DETECTION CONDITION | • Base unit detects communication error with CD changer (upper module)
POSSIBLE CAUSE | • Malfunction of connectors between base unit and CD changer (upper module) • CD changer (upper module) malfunction • Base unit malfunction

Diagnostic procedure

STEP | INSPECTION | ACTION
--- | --- | ---
1 | INSPECT CONNECTOR • Remove CD changer (upper module) and inspect connector for the following.

  - Deformation of pin
  - Poor connection of female terminal
  - Pinching of foreign material

• Is connector okay?
Yes
Go to next step.
No | Repair connector, then go to next step.
2 | VERIFY THAT CD CHANGER (UPPER MODULE) IS INSTALLED WITH BASE UNIT • Install CD changer (upper module) and verify its installation condition. • Is CD changer (upper module) securely installed? | Yes | Go to next step.
No | Securely install CD changer (upper module), then go to next step.
3 | INSPECT CD CHANGER (UPPER MODULE) • Clear DTC. • Turn ignition switch to ACC or ON position and hold for 3 seconds or more. • Start on-board diagnostic test mode. • Is DTC 06 ERR10 or 06:Er10 displayed? | Yes | Replace base unit and CD changer (upper module).
No | Troubleshooting completed.