#
CARGO COMPARTMENT LIGHT REMOVAL/INSTALLATION

BME091851441201

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | Cargo compartment light (See Cargo Compartment Light Removal Note.)
2 | Connector

## Cargo Compartment Light Removal Note

1. Insert a tape-wrapped flathead screwdriver into the service hole.

2. Press the clip with the flathead screwdriver to remove the cargo compartment light.