#
DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION

BME081057010201

  Warning

  • Handling the air bag module improperly can accidentally deploy the air bag module, which may seriously injure you. Read the service warnings and cautions before handling the air bag module. (See SERVICE WARNINGS.)

1. Turn the ignition switch to LOCK position.

2. Disconnect the negative battery cable and wait for 1 min or more.

3. Remove in the order indicated in the table.

1 | Cover
2 | Bolt
3 | Connector (See Connector Removal Note)
4 | Driver-side air bag module

4. Install in the reverse order of removal.

5. Turn the ignition switch to ON position.

6. Verify that the air bag system warning light illuminates for approx. 6 s and then goes off.

  • If the air bag system warning light does not operate in the manner described above, there are malfunctions in the system. Inspect the system using the on-board diagnostic.

## Connector Removal Note

1. Using a flathead screwdriver, pry out the connector stopper plate.

2. Disconnect the connector.