#
ENGINE COOLANT TEMPERATURE (ECT) SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME014018841W03

  Warning

  • When the engine is hot, it can badly burn. Turn off the engine and wait until it is cool before removing the ECT sensor.

1. Disconnect the negative battery cable.

2. Drain the engine coolant. (See ENGINE OIL REPLACEMENT.)

3. Remove the common rail. (See SUPPLY PUMP REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

4. Remove in the order indicated in the table.

1 | ECT sensor
2 | Gasket

5. Install in the reverse order of removal.