#
DTC TABLE

BME080201046202
• DTCs are common for present and past malfunction diagnosis.

  Note

  • After a new SAS unit is installed, the air bag system warning light continuously flashes when the ignition switch is turned to the ON position. This is the deployment authorization standby code output by the SAS unit. Perform the deployment authorization and restore the system to an operational state.
  • If the air bag system warning light does not illuminate or remains illuminated when the ignition switch is turned to the ON position, inspect and repair the air lighting circuit system of air bag system warning light and then confirm that the air bag system warning light is operational.

DTC | Output signal | Malfunction location
--- | --- | ---
1 |  | SAS unit connector poor connection
2 |  | SAS unit
3 |  | Power supply of SAS unit
6 |  | Driver-side air bag module system
7 |  | Passenger-side air bag module system
11 |  | Driver-side pre-tensioner seat belt system
12 |  | Passenger-side pre-tensioner seat belt system
22 |  | Driver-side side air bag sensor system (Internal circuit abnormal)
25 |  | Driver-side side air bag sensor system (Communication error)
26 |  | Driver-side side air bag module system
32 |  | Passenger-side side air bag sensor system (Internal circuit abnormal)
35 |  | Passenger-side side air bag sensor system (Communication error)
37 |  | Passenger-side side air bag module system
44 |  | Short to ground in wiring harness between SAS unit and occupancy sensor
45 |  | Open circuit in wiring harness between SAS unit and occupancy sensor
46 |  | Passenger-side air bag cut-off indicator light system
47 |  | Occupancy sensor (Occupancy detection part)
48 |  | Occupancy sensor (Child restraint seat detection part)
91 |  | Air bag system warning light system
- | Continuously flashes | Deployment authorization standby code