#
REAR A/C UNIT DISASSEMBLY/ASSEMBLY

BME071100103W02

1. Disassemble in the order indicated in the table.

2. Assemble in the reverse order of disassembly.

.

1 | Rear airflow mode actuator (equipped with rear A/C and heater)
2 | Rear air mix actuator (equipped with rear A/C and heater)
3 | Rear resistor
4 | Rear blower relay
5 | Rear blower motor
6 | Rear heater core (except rear A/C only)
7 | Rear expansion valve (except rear heater only)
8 | Case (left)
9 | Case (right)
10 | Rear evaporator (except rear heater only) (See Rear Evaporator Assembly Note)
11 | Airflow mode door
12 | Air mix door

## Rear Evaporator Assembly Note

1. When installing a new rear evaporator, add ND-OIL8 compressor oil from the inlet.

Supplemental amount

  40 ml {40 cc, 1.4 fl oz}