#
SUSPENSION SPECIFICATIONS

BME020001013T02

## Suspension

Item | Specification
--- | ---
Front suspension | Suspension type | Strut
Shock absorber type | Cylindrical, double-acting (low-pressure gas charged)
Spring type | Coil spring
Stabilizer | Type | Torsion bar
Diameter | (mm {in}) | 18.0 {0.71}
Wheel alignment (Unloaded*1) | Maximum steering angle [Tolerance ±3°] | Inner | 37°06'
Outer | 32°00'
Total toe-in | (mm {in}) | Rim inner: 1±3 {0.04±0.12}, Tire: 2±4 {0.08±0.16}
(degree) | 0°11'±0°22'
Camber angle*2 [Tolerance ±1°] | -0°14'
Caster angle*2 [Tolerance ±1°] | 2°02'
Steering axis inclination | 11°11'
(Reference value)
Rear suspension | Suspension type | Torsion beam
Shock absorber type | Cylindrical, double-acting (low-pressure gas charged)
Spring type | Coil spring
Stabilizer | Type | Torsion bar
Diameter | (mm {in}) | 34.0 {1.34}
Wheel alignment (Unloaded*1) | Total toe-in | (mm {in}) | Rim inner: 2±3 {0.08±0.12}, Tire: 3±4 {0.12±0.16}
(degree) | 0°17'±0°22'
Camber angle*2 (Reference value) [Tolerance ±1°] | -1°
Thrust angle (Reference value) [Tolerance ±48'] | 0°

  *1 :
Fuel tank full. Engine coolant and engine oil are at specified levels. Spare tire, jack and tools are in designated positions.
  *2 :
Difference between left and right must not exceed 1°30' .

## Wheel and Tire

### Standard tire

European (L.H.D. U.K.) specs.

Item | Specification
--- | ---
Tire | Size | 205/65R15 94T | 215/60R16 95H
Wheel | Size | 15 × 6J | 15 × 6JJ | 16 × 6 1/2J
Material | Aluminum alloy | Steel | Steel, Aluminum alloy
Offset | (mm {in}) | 50 {1.97}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}

Australian, General (L.H.D. R.H.D.) specs.

Item | Specification
--- | ---
Tire | Size | 205/65R15 94H | 215/60R16 95H | 215/60R17 96H
Wheel | Size | 15 × 6J | 15 × 6JJ | 16 × 6 1/2J | 17 × 7J
Material | Aluminum alloy | Steel | Aluminum alloy
Offset | (mm {in}) | 50 {1.97}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}

### Temporary spare tire

European (L.H.D. U.K.) specs.

Item | Specification
--- | ---
Tire | Size | T135/90D15 | T145/80D16
Wheel | Size | 15 × 4T | 16 × 4T
Material | Steel
Offset | (mm {in}) | 45 {1.77}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}

Australian, General (L.H.D. R.H.D.) specs.

Item | Specification
--- | ---
Tire | Size | T135/90D15 | T145/80D16
Wheel | Size | 15 × 4T | 16 × 4T
Material | Steel
Offset | (mm {in}) | 35 {1.38} | 45 {1.77}
Pitch circle diameter | (mm {in}) | 114.3 {4.50}