#
AIR CLEANER ELEMENT INSPECTION [L3]

BME011313300201

1. Remove the air cleaner element. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L3].)

2. Inspect the following items:

  • If there is any malfunction, clean or replace the air cleaner element.
  • If the replacement interval has come, replace the air cleaner element.

  - Is the air cleaner element soiled, damaged, or bent?
  - Are the air cleaner case and the air cleaner element correctly sealed?
  - Is the correct air cleaner element installed?