#
PRIMARY SHAFT COMPONENTS DISASSEMBLY

BME051517201M02

1. Disassemble in the order indicated in the table.

1 | Primary shaft rear bearing adjust shim
2 | Oil channel
3 | Primary shaft rear bearing (See Primary Shaft Rear Bearing Disassembly Note.)
4 | Snap ring
5 | Primary shaft bearing spacer (See Primary Shaft Bearing Spacer and 5th Gear Stopper Disassembly Note.)
6 | 5th gear stopper
7 | 5th clutch hub set (See 5th Clutch Hub Set, 5th Synchronizer Ring and 5th Gear Disassembly Note.)
8 | 5th synchronizer ring
9 | 5th gear
10 | 5th needle bearing
11 | 5th bushing (See 5th Bushing, Thrust Washer, 4th Gear, 4th Needle Bearing, 4th Bushing, 4th Synchronizer Ring, 3rd/4th Clutch Hub Set, 3rd Synchronizer Ring and 3rd Gear Disassembly Note.)
12 | Thrust washer
13 | 4th gear
14 | 4th needle bearing
15 | 4th bushing
16 | 4th synchronizer ring
17 | 3rd/4th clutch hub set
18 | 3rd synchronizer ring
19 | 3rd gear
20 | 3rd needle bearing
21 | Primary shaft
22 | Primary shaft front bearing (See Primary Shaft Front Bearing Disassembly Note.)
23 | Synchronizer key spring (5th)
24 | 5th synchronizer key
25 | 5th clutch hub and sleeve
26 | 3rd/4th synchronizer key
27 | 3rd/4th clutch hub and sleeve
28 | Synchronizer key spring (3rd/4th)

## Primary Shaft Rear Bearing Disassembly Note

1. Remove the bearing using the SSTs.

## Primary Shaft Bearing Spacer and 5th Gear Stopper Disassembly Note

1. Remove the primary shaft bearing spacer and 5th gear stopper at the same time using the SSTs.

## 5th Clutch Hub Set, 5th Synchronizer Ring and 5th Gear Disassembly Note

1. Remove the 5th clutch hub set, 5th synchronizer ring and 5th gear at the same time using the SSTs.

## 5th Bushing, Thrust Washer, 4th Gear, 4th Needle Bearing, 4th Bushing, 4th Synchronizer Ring, 3rd/4th Clutch Hub Set, 3rd Synchronizer Ring and 3rd Gear Disassembly Note

1. Remove the 5th bushing, thrust washer, 4th gear, 4th needle bearing, 4th bushing, 4th synchronizer ring, 3rd/4th clutch hub set, 3rd synchronizer ring and 3rd gear at the same time using the SSTs.

## Primary Shaft Front Bearing Disassembly Note

1. Remove the primary shaft front bearing using the SST.