#
FUEL GAUGE SENDER UNIT REMOVAL/INSTALLATION

BME092260960W01

## MZR-CD (RF Turbo)

  Warning

  • Repairing a fuel tank that has not been properly steam cleaned can be dangerous. Explosion or fire may cause death or serious injury. Always properly steam clean a fuel tank before repairing it.
  • fuel line spills and leakage are dangerous. Fuel can also irritate skin and eyes. To prevent this, do not damage the sealing surface of the fuel gauge sender unit when removing or installing.

1. Level the vehicle.

2. Complete the "BEFORE REPAIR PROCEDURE". (See BEFORE REPAIR PROCEDURE [MZR-CD (RF Turbo)].)

3. Disconnect the negative battery cable.

4. Remove the front seats.

5. Remove the front scuff plates.

6. Remove the rear scuff plates.

7. Remove the console lower cover.

8. Loosen the parking brake lever installation bolts.

9. Partially peel back the floor covering until the service hole cover appears.

10. Remove the service hole cover.

11. Remove in the order indicated in the table.

1 | Screw
2 | Fuel hose
3 | Connector
4 | Fuel gauge sender unit

12. Install in the reverse order of removal.

13. Complete the "AFTER REPAIR PROCEDURE". (See AFTER REPAIR PROCEDURE [MZR-CD (RF Turbo)].)