#
EXHAUST SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME011500115204

  Warning

  • When the engine and exhaust system are hot, they can cause severe burns or injury. Turn off the engine and wait until they are cool before removing the exhaust system.

1. Disconnect the negative battery cable.

2. Remove in the order indicated in the table.

3. Install in the reverse order of removal.

1 | After silencer
2 | Main silencer
3 | Oxidation catalytic converter
4 | Flexible pipe
5 | Warm up oxidation catalytic converter (See Warm Up Oxidation Catalytic Converter Removal Note)
6 | Turbocharger insulator No. 1
7 | Turbocharger insulator No. 2
8 | Exhaust manifold insulator
9 | Oil pipe
10 | Water hose (See Water Hose Removal Note)
11 | Turbocharger (See Turbo charger Removal Note)
12 | Exhaust manifold (See Exhaust Manifold Removal Note) (See Exhaust Manifold Installation Note)

## Warm Up Oxidation Catalytic Converter Removal Note

1. Remove the joint shaft before removing the warm up oxidation catalytic converter. (See JOINT SHAFT (MZR-CD (RF Turbo)) REMOVAL/INSTALLATION.)

## Water Hose Removal Note

1. Drain the engine coolant. (See ENGINE COOLANT REPLACEMENT [MZR-CD (RF Turbo)].)

## Turbo charger Removal Note

1. Remove the air pipe and the air hose before removing the turbocharger. (See INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

## Exhaust Manifold Removal Note

1. Remove the EGR pipe before removing the exhaust manifold. (See EGR VALVE REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

## Exhaust Manifold Installation Note

1. Tighten the exhaust manifold installation nuts in the order shown.