#
SLIDING DOOR ADJUSTMENT

BME091173002W03

1. Measure the gap and height between the sliding door and the body.

2. If not as specified, loosen the roller installation bolts or the door lock striker installation screws, and reposition the door.

Clearance

  a: 3.5-6.5 mm {0.14-0.25 in}
  b: -1.5-1.5 mm {-0.05-0.05 in}
  c: 3.5-6.5 mm {0.14-0.25 in}
  d: -1.5-1.5 mm {-0.05-0.05 in}
  e: 0-1.0 mm {0-0.03 in}

3. Tighten the bolts or screws.