#
DOOR KEY CYLINDER SWITCH REMOVAL/INSTALLATION

BME091475911W01

1. Fully raise the door glass.

2. Disconnect the negative battery cable.

3. Remove the door screen.

4. Disconnect the door key cylinder switch connector.

5. Disconnect the rods.

6. Remove the nuts, and remove the outer handle.

7. Remove the pin, and remove the door key cylinder switch from the outer handle.

8. Install in the reverse order of removal.