#
NO.2 MIL ILLUMINATES [MZR-CD (RF Turbo)]

BME010300103273

2 | MIL ILLUMINATES
--- | ---
DESCRIPTION | • MIL illuminates incorrectly.
POSSIBLE CAUSE | • PCM illuminates for emission-related concern (DTC is stored in PCM) • Instrument cluster malfunction

  Note

  • If MIL blinks at steady rate, misfire condition could possibly exist.

Diagnostic procedure

STEP | INSPECTION | RESULTS | ACTION
--- | --- | --- | ---
1 | Connect the WDS or equivalent to the DLC-2. Turn engine switch to the ON position. Retrieve any DTC. Is DTC displayed? | Yes | DTC is displayed: • Go to the applicable DTC inspection. (See DTC TABLE [MZR-CD (RF Turbo)].)
No | No DTC is displayed: • Inspect the instrument cluster operation.
2 | Verify test results. • If normal, return to diagnostic index to service any additional symptoms. • If malfunction remains, replace the PCM. (See PCM REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)