#
FOREWORD

BME010266350202

## Outline

• There are two on-board diagnostic functions: Operation mode, which inspects for and indicates correct operation of the input signals to the control module, and Condition detection mode, which indicates troubles in the system.
• The two functions can be done using either of the following methods:

  - Verifying the flashing pattern of the cruise set indicator light in the instrument cluster.
  - Verifying the output of the DLC using the SST (WDS or equivalent).

## Inspection Order