#
AUDIO CONTROL SWITCH REMOVAL/INSTALLATION

BME092000148201

  Note

  • The audio control switch and the cruise control switch use a common connector.

1. Disconnect the negative battery cable.

2. Remove the driver-side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

3. Remove the steering wheel.

4. Remove in the order indicated in the table.

1 | Bolt
2 | Bracket
3 | Screw
4 | Cover
5 | Screw
6 | Audio control switch/cruise control switch

5. Install in the reverse order of removal.