#
FOREWORD [L3]

BME010200102213
• When the customer reports a vehicle malfunction, check the malfunction indicator lamp (MIL) indication and diagnostic trouble code (DTC), then diagnose the malfunction according to the following flowchart.

  - If a DTC exists, diagnose by following the applicable DTC inspection. (See DTC TABLE [L3].)
  - If no DTC exists and the MIL does not illuminate or flash, diagnose by following the applicable symptom troubleshooting. (See ENGINE SYMPTOM TROUBLESHOOTING [L3].)
  * :
Malfunction Indicator lamp (MIL), Generator Warning Light, Security Light