#
DRIVE PLATE REMOVAL/INSTALLATION [JA5A-EL]

BME051719020202

1. Remove in the order indicated in the table.

2. Install in the reverse order of removal.

1 | Drive plate mounting bolts (See Drive Plate Mounting Bolts Removal Note.) (See Drive Plate Mounting Bolts Installation Note.)
2 | Backing plate
3 | Drive plate

## Drive Plate Mounting Bolts Removal Note

1. Set the SST or equivalent against the drive plate.

2. Remove the bolts and the drive plate.

## Drive Plate Mounting Bolts Installation Note

1. Set the SST or equivalent against the drive plate.

2. Tighten the drive plate mounting bolts in two or three steps in the order as shown in the figure.

Tightening torque

  73-87 N·m {7.4-8.9 kgf·m, 54-64 ft·lbf}