#
FRONT DOOR LOCK ACTUATOR INSPECTION

BME091458310202

## Door Lock Actuator

1. Remove the front door trim.

2. Partially peel off the door screen.

3. Disconnect the front door lock actuator connector.

4. Apply battery positive voltage to the front door lock actuator terminals and inspect the operation of the front door lock actuator.

  • If not as specified, replace the front door lock actuator.

Without double locking system

Connection | Actuator operation
--- | ---
B+ | GND
B | E | Lock
E | B | Unlock

With double locking system

Connection | Actuator operation
--- | ---
B+ | GND
E | B | Lock
E | C | Double lock
B and C | E | Unlock

## Door Lock-link Switch

1. Remove the front door trim.

2. Turn the door screen over.

3. Disconnect the front door lock actuator connector.

4. Inspect for continuity between the door lock-link switch terminals using an ohmmeter.

  • If not as specified, replace the front door lock actuator.

Driver's side

Passenger's side (with theft-deterrent system)