#
SLIDING DOOR CIRCUIT CONTACT INSPECTION

BME0911739A0W02

## Door Side

1. Disconnect the negative battery cable.

2. Remove the sliding door trim.

3. Disconnect the sliding door circuit contact connector.

4. Inspect for continuity between the sliding door circuit contact terminals using an ohmmeter.

  • If not as specified, replace the sliding door circuit contact.

## Body Side

1. Disconnect the negative battery cable.

2. Remove the B-pillar lower trim.

3. Disconnect the sliding door circuit contact connector.

4. Inspect for continuity between the sliding door circuit contact terminals using an ohmmeter.

  • If not as specified, replace the sliding door circuit contact.