#
NEUTRAL SWITCH INSPECTION [L3]

BME014017640W01

  Note

  • Perform the following inspection only when directed.

## Continuity Inspection

1. Disconnect the negative battery cable.

2. Remove the neutral switch. (See MANUAL TRANSAXLE REMOVAL/INSTALLATION [G15M-R].)

3. Inspect for continuity between the neutral switch terminals using an ohmmeter.

  • If the neutral switch is okay, but CPP/PNP PID value is out of specification, carry out of the "Circuit Open/Short Inspection".
  • If not as specified, replace the neutral switch.

Specification

## Circuit Open/Short Inspection

1. Disconnect the PCM connector. (See PCM REMOVAL/INSTALLATION [L3].)

2. Inspect the following harness for open or short. (Continuity check)

### Open circuit

  • Neutral switch terminal A (harness-side) and PCM terminal 1W (harness-side)
  • Neutral switch terminal B (harness-side) and body GND

### Short circuit

  • Neutral switch terminal A (harness-side) and body GND