#
DUAL PROPORTIONING VALVE INSPECTION

BME041143900W01

## Without ABS

1. Connect the SSTs to the brake pipes as shown in the figure.

2. Bleed the air from the brake system.

3. Measure the fluid pressure of the master cylinder and the rear brake.

  • If not within the specification, replace the dual proportioning valve.

Fluid pressure

kPa {kgf/cm2, psi}

A | A' | B | B'
--- | --- | --- | ---
3430 {34.98, 497.4} | 3430 {34.98, 497.4} ±300 {3.06, 43.5} | 5880 {59.96, 852.6} | 4165 {42.47, 603.9} ±425 {4.33, 61.6}