#
AUTOMATIC TRANSAXLE FEATURES

B3E051701030A02

Realization of excellent shift quality | Electronic pressure-adjusting control of line pressure by a liner type solenoid (pressure control solenoid) adopted Electronic control (direct electric shift control) of clutch pressure by duty-cycle type solenoids (shift solenoid A, B, and C) adopted
Centrifugal balance clutch chamber adopted
High efficiency, compactness, and light weight | Miniature trochoid gear type oil pump with torque converter direct drive adopted Bonded seal piston adopted Tow-step final gear drive mechanism adopted
Improved reliability, reduced NVH (noise, vibration and harshness) | Double arranged gears with a single planetary gear unit adopted