#
QUARTER WINDOW GLASS INSTALLATION

BME091262580W02

  Caution

  • Keep the area free of dirt and grease, and do not touch the surface or the primer may not properly bond to the surface of the molding, which may cause leaks to occur.

1. Apply primer to the edge of the quarter window glass and the inside of the quarter window molding, and allow the primer to dry for approximately 30 minutes.

2. Apply sealant to the inside of the quarter window molding.

3. Fit the quarter window molding onto the glass.

4. Install the screws and the lock.

5. Install the screws and nuts, then the quarter window glass.

6. Install the D-pillar trim.

7. Install the C-pillar trim.