#
CLUTCH SWITCH INSPECTION [MZR-CD (RF Turbo)]

BME014018660W02

  Note

  • Perform the following test only when directed.

## Continuity Inspection

1. Inspect continuity between the clutch switch terminals using an ohmmeter.

  • If the clutch switch is okay, but the CPP PID is out of specification, perform the "Circuit Open/Short Inspection"
  • If not as specified, replace the clutch switch.

Specification

## Circuit Open/Short Inspection

1. Inspect for open/short circuit in the following wiring harnesses.

  • If there is open/short circuit, repair or replace wiring harnesses.

### Open circuit

  • Signal circuit
  - Clutch switch terminal C and PCM terminal 33
  • GND circuit
  - Clutch switch terminal E and GND

### Short circuit

  • Signal circuit
  - Clutch switch terminal C and PCM terminal 33 to GND.