#
SUNROOF UNIT DISASSEMBLY/ASSEMBLY

BME091569850W02

1. Disconnect the negative battery cable.

2. Remove the deflector.

3. Remove the glass panel.

4. Disassemble in the order indicated in the table.

5. Assemble in the reverse order of disassembly.

1 | Drip rail
2 | Position plate
3 | Slider (See Slider Disassembly Note.)
4 | Rear Stopper
5 | Sunshade
6 | Sunroof motor
7 | Sunroof relay
8 | Drive unit
9 | Decoration link (See Decoration Link Assembly Note.)
10 | Guide (See Guide Disassembly Note.) (See Guide Assembly Note.)
11 | Set plate A
12 | Set plate B
13 | Front stopper
14 | Frame
15 | Stopper

## Slider Disassembly Note

1. Remove the screw.

2. Slide the slider rearward, and remove it from the sunroof frame.

## Guide Disassembly Note

1. Slide the guide rearward, and remove it from the sunroof frame.

## Decoration Link Assembly Note

1. Set the pin in the decoration link.

## Guide Assembly Note

1. Move the guide by hand until it comes to the front stopper.

2. Move the guide by hand until center of pin comes between mark A and B.