#
BONNET ADJUSTMENT

BME091052310W02

1. Measure the gap and height between the bonnet and the body.

  • If not as specified, adjust the gap and height. (See Gap Adjustment.) (See Height Adjustment.)

Clearance

  a: 4.0-8.0 mm {0.16-0.31 in}
  b: 4.0-8.0 mm {0.16-0.31 in}
  c: Bumper should not pass bonnet.
  d: 4.0-8.0 mm {0.16-0.31 in}
  e: 3.0-5.0 mm {0.12-0.19 in}
  f: -1.5-0.5 mm {-0.059-0.019 in}

## Gap Adjustment

1. Loosen the bonnet installation bolts and reposition the bonnet.

2. Tighten the bolts.

## Height Adjustment

1. Turn the stop rubber to adjust the height of the bonnet.