#
AIR BAG MODULE AND PRE-TENSIONER SEAT BELT DEPLOYMENT PROCEDURES

BME081057000W05

  Warning

  • Live (undeployed) air bag module and pre-tensioner seat belt may accidentally deploy when it is disposed of and cause serious injury. Do not dispose of a live (undeployed) air bag module and pre-tensioner seat belt. If the SSTs (Deployment tool and Adapter harness) are not available, consult the nearest Mazda representative for assistance.

  Caution

  • Deploying the air bag modules and pre-tensioner seat belts inside the vehicle may cause damage to the vehicle interior. When the vehicle is not to be scrapped, always deploy the air bag modules and pre-tensioner seat belts outside the vehicle.

• When the vehicle is to be scrapped, deploy the air bag modules and pre-tensioner seat belts inside the vehicle. (See Deployment Procedure for Inside of Vehicle (Only When Vehicle Is To Be Scrapped).)
• When the vehicle is not to be scrapped, deploy the air bag modules and pre-tensioner seat belts outside the vehicle. (See Deployment Procedure for Outside of Vehicle.)

  Note

  • When disposing of deployed air bag module and pre-tensioner seat belt, refer to the disposal procedure, (See AIR BAG MODULE AND PRE-TENSIONER SEAT BELT DISPOSAL PROCEDURES.)

## Deployment Procedure for Inside of Vehicle (Only When Vehicle Is To Be Scrapped)

1. Inspect the SST (Deployment tool). (See INSPECTION OF SST (DEPLOYMENT TOOL).)

2. Move the vehicle to an open space, away from strong winds, and close all of the vehicle's doors and windows.

3. Turn the ignition switch to LOCK position.

4. Disconnect the negative battery cable and wait for more than 1 minute.

5. Follow the appropriate procedure for deploying the driver-side air bag module, passenger-side air bag module, side air bag module, or pre-tensioner seat belt.

### Driver-side air bag module

1. Remove the column cover.

2. Disconnect the clock spring connector.

3. Connect the SST (Adapter harness) to the clock spring as shown in the figure.

4. Connect the SST (Deployment tool) to the SST (Adapter harness).

5. Connect the red clip of the SST (Deployment tool) to the positive battery terminal and the black clip to the negative battery terminal.

6. Verify that the red light on the SST (Deployment tool) is illuminated.

7. Make sure all persons are standing at least 6 m {20 ft} away from the vehicle.

8. Press the activation switch on the SST (Deployment tool) to deploy the driver-side air bag module.

### Passenger-side air bag module

1. Remove the glove compartment.

2. Disconnect the passenger-side sir bag module connector.

3. Connect the SST (Adapter harness) to the passenger-side air bag module as shown it the figure.

4. Connect the SST (Deployment tool) to the SST (Adapter harness).

5. Connect the red clip of the SST (Deployment tool) to the positive battery terminal and the black clop to the negative battery terminal.

6. Verify that the red light on the SST (Deployment tool) is illuminated.

7. Make sure all persons are standing at least 6 m {20 ft} away from the vehicle.

8. Press the activation switch on the SST (Deployment tool) to deploy the passenger-side air bag module.

### Side air bag module

1. Disconnect the side air bag module connector.

2. Connect the SST (Adapter harness) to the side air bag module.

3. Connect the SST (Deployment tool) to the SST (Adapter harness).

4. Connect the red clip of the SST (Deployment tool) to the positive battery terminal and the block clop to the negative battery terminal.

5. Verify that the red light on the SST (Deployment tool) is illuminated.

6. Make sure all persons are standing at least 6 m {20 ft} from the vehicle.

7. Press the activation switch on the SST (Deployment tool) to deploy the side air bag module.

### Pre-tensioner seat belt

1. Remove the B-pillar lower trim.

2. Remove the pre-tensioner seat belt and connect the SST (Adapter harness) to it as shown in the figure. (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

3. Install the pre-tensioner seat belt.

4. Connect the SST (Deployment tool) to the SST (Adapter harness).

5. Connect the red clip of the SST (Deployment tool) to the positive battery terminal and the black clip to the negative battery terminal.

6. Verify that the red light on the SST (Deployment tool) is illuminated.

7. Make sure all persons are standing at least 6 m {20 ft} from the vehicle.

8. Press the activation switch on the SST (Deployment tool) to deploy the pre-tensioner seat belt.

## Deployment Procedure for Outside of Vehicle

1. Inspect the SST (Deployment tool). (See INSPECTION OF SST (DEPLOYMENT TOOL).)

2. Turn the ignition switch to LOCK position.

3. Disconnect the negative battery cable and wait for more than 1 minute.

4. Follow the appropriate procedure for deploying the driver-side air bag module, passenger-side air bag module, side air bag module, or pre-tensioner seat belt.

### Driver-side air bag module

1. Remove the driver-side air bag module. (See DRIVER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

2. Install the bolts to the driver-side air bag module.

  Warning

  • If the air bag module is not properly installed to the tire wheel, serious injury may occur when the module is deployed. When installing the air bag module to the tire wheel, make sure the module is facing up.

3. Place the driver-side air bag module on the center of the tire wheel with the module facing up. To secure the air bag module to the tire wheel, wrap the wire harness through the wheel and around the bolt at least four times.

4. Connect the SST (Adapter harness) to the driver-side air bag module as shown in the figure,

5. Stack three tires on top of the tire with the air bag module. Stack another tire that has a wheel on top of the four tires.

6. Tie all tires together with wire.

7. Connect the SST (Deployment tool) to the SST (Adapter harness).

8. Connect the red clip of the SST (Deployment tool) to the positive battery terminal and the black clip to the negative battery terminal.

9. Verify that the red light on the SST (Deployment tool) is illuminated.

10. Make sure all persons are standing at least 6 m {20 ft} away from the vehicle.

11. Press the activation switch on the SST (Deployment tool) to deploy the driver-side air bag module.

### Passenger-side air bag module

1. Remove the passenger-side air bag module. (See PASSENGER-SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

2. Install the bolts to the passenger-side air bag module.

  Warning

  • If the air bag module ia not properly installed to the tire, serious injury may occur when the module is deployed, When installing the air bag module to the tire, make sure the module is facing the center of the tire.

3. Tie the passenger-side air bag module to the tire with the module facing the center of the tire. Wrap the wire harness through the tire and around the bolts at least four times.

4. Connect the SST (Adapter harness) to the passenger-side air bag module as shown in the figure.

5. Stack the tire with the passenger-side air bag module on top of two tires. Stack another tire that has a wheel on top of the four tires.

6. Tie all tires together with wire.

7. Connect the SST (Deployment tool) to the SST (Adapter harness).

8. Connect the red clip of the SST (Deployment tool) to the positive battery terminal and the black clip to the negative battery terminal.

9. Verify that the red light on the SST (Deployment tool) is illuminated.

10. Make sure all persons are standing at least 6 m {20 ft} away from the vehicle.

11. Press the activation switch on the SST (Deployment tool) to deploy the passenger-side air bag module.

### Side air bag module

1. Remove the side air bag module. (See SIDE AIR BAG MODULE REMOVAL/INSTALLATION.)

2. Install the nuts to the side air bag module.

  Warning

  • If the air bag module is not properly installed to the tire, serious injury may occur when the module is deployed. When installing the air bag module to the tire, make sure the module is facing the center of the tire.

3. Tie the side air bag module to the tire with the module facing the center of the tire. Wrap the wire harness through the tire and around the nuts at least four times.

4. Connect the SST (Adapter harness) to the side air bag module as shown in the figure.

5. Stack the tire with the side air bag module on top of two tires. Stack a tire on top of three tires. Stack another tire that has a wheel on top of the four tires.

6. Tie all tires together with wire.

7. Control the SST (Deployment tool) to the SST (Adapter harness).

8. Connect the red clip of the SST (Deployment tool) to the positive battery terminal and the black clip to the negative battery terminal.

9. Verify that the red light on the SST (Deployment tool) is illuminated.

10. Make sure all persons are standing at least 6 m {20 ft} from the vehicle.

11. Press the activation switch on the SST (Deployment tool) to deploy the side air bag module.

### Pre-tensioner seat belt

1. Remove the pre-tensioner seat belt. (See FRONT SEAT BELT REMOVAL/INSTALLATION.)

  Warning

  • If the pre-tensioner seat belt is not properly installed to the tire, serious injury may occur when the pre-tensioner part is deployed. When installing the pre-tensioner seat belt to the tire, make sure the pre-tensioner part is inside the tire.

2. Connect the SST (Adapter harness) to the pre-tensioner seat belt as shown in the figure.

3. With the pre-tensioner part inside the tire, tie the pre-tensioner seat belt to the tire. Wrap the wire harness through the tire and around the pre-tensioner seat belt at least four times.

4. Stack the tire with the pre-tensioner seat belt on top of two tires. Stack a tire on top of the three tires. Stack another tire that has a wheel on top of the four tires.

5. Tie all tires together with wire.

6. Connect the SST (Deployment tool) to the SST (Adapter harness).

7. Connect the red clip of the SST (Deployment tool) to the positive battery terminal and the black clip to the negative battery terminal.

8. Verify that the red light on the SST (Deployment tool) is illuminated.

9. Make sure all persons are standing at least 6 m {20 ft} from the vehicle.

10. Press the activation switch on the SST (Deployment tool) to deploy the pre-tensioner seat belt.