#
SHIFT CONTROL DESCRIPTION [JA5A-EL]

BME051718901T03

## Outline

### Features

  • The TCM selects and determines the shift diagram based on the results of the range and driving mode judgements. Then, based on the shift diagram, the TCM sends the signal to the duty-cycle type solenoid valves and the ON/OFF type solenoid valves, according to the VSS signal and the throttle opening signal, to perform shifting.

### Construction (system diagram)

## Operation

### Range determination

  • Each range is determined by operating the selector lever, and switching ON/OFF the switch in the TR switch internal circuit. The present range is detected according to the ON/OFF signal of the switch.
  • The following switches are built into the TR switch, and determine each range when the switch is on.
  P position switch
  R position switch
  N position switch
  D range switch
  S range switch
  L range switch