#
DTC 05

BME010266350211

DTC 05 | Brake switch
--- | ---
DETECTION CONDITION | • Voltage detected at cruise actuator connector terminal C is always approximately 0 V.
POSSIBLE CAUSE | • Cruise actuator malfunction

Diagnostic procedure

INSPECTION | ACTION
--- | ---
INSPECT DTC FOR OPERATION MODE • Was operation mode for DTC 31 performed? | Yes | Perform operation mode for DTC 31 on-board diagnostic again. Even if no malfunctions are detected in operation mode, if DTC 05 is indicated in condition detection mode on-board diagnostic, replace cruise actuator. (See CRUISE ACTUATOR REMOVAL/INSTALLATION)
No | Perform operation mode for DTC 31.