#
CRANKSHAFT POSITION (CKP) SENSOR REMOVAL/INSTALLATION [MZR-CD (RF Turbo)]

BME014011430201

  Caution

  • When foreign material, such as iron chips, gets on the CKP sensor, it can cause abnormal output from the sensor because of flux turbulence and adversely affect engine control. Be sure there is no foreign material on the CKP sensor when replacing.
  • Do not forcefully pull the wiring harness of the CKP sensor. Doing so will break the harness.

1. Disconnect the negative battery cable.

2. Remove the crankshaft pulley. (See TIMING BELT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

3. Remove the lower timing belt cover. (See TIMING BELT REMOVAL/INSTALLATION [MZR-CD (RF Turbo)].)

4. Remove in the order indicated in the table.

1 | CKP sensor installation bolt
2 | CKP sensor

5. Install in the reverse order of removal.