#
PCV VALVE INSPECTION [L3]

BME011613890W01

1. Disconnect the negative battery cable.

2. Remove the intake maniforld.(see INTAKE-AIR SYSTEM REMOVAL/INSTALLATION [L3].)

3. Remove the PCV valve.

4. Blow through the valve and verify that air flows as specified.

  • If not as specified, replace the PCV valve.

Specification

Condition | Airflow
--- | ---
Air applied from port A to B | Yes
Air applied from port B to A | No